Band Steering

Band steering allows the device to determine if a connected client is dual-band capable. If so, the client can be forced to use the less congested 5GHz network.

This is done by blocking the client from connecting to the 2.4GHz network.