Latency Path

The DSL Latency Path comes in three modes: Path 1 (Fast), Path 2 (Interleaved) and Both 1 & 2. Fast is used for applications sensitive to delay. Interleaved suits applications sensitive to errors.