Loop Attenuation

Loop Attenuation is a measure of the quality of the line - how much the signal weakens over the loop.

Attenuation is measured in Decibel (dB). A value betwen 20dB-45dB can be considered normal.