LSAP

Link Service Access Point (LSAP) fields are used to identify which protocol handler should process an incoming frame.

LSAP fields allow the receiving node to pass each received frame to an appropriate device driver which understands given protocol.