VC-MUX

Virtual Circuit Multiplexing (VC-MUX) is a method for identifying the protocol carried in frames used in ATM.

Using virtual circuit multiplexing, hosts agree on the high-level protocol for a given circuit. Each high-level protocol requires a separate virtual circuit.